Example Code (HU/TBM):

    /**********************************************************************************************
     * This example code is provided for illustrative purposes only and provided 'AS IS' without
     * warranty of any kind.
     *
     * Copyright ©2014 Chrysler Group LLC.  All Rights Reserved.  All information contained herein is,
     * and remains the property of Chrysler Group LLC and its suppliers, if any.  The intellectual and
     * technical concepts contained herein are proprietary to Chrysler Group LLC and its suppliers
     * and may be covered by U.S. and Foreign Patents, patents in process, and are protected by trade
     * secret or copyright law. Dissemination of this information or reproduction of this material is
     * strictly forbidden unless prior written permission is obtained from Chrysler Group LLC.
     *
     * Chrysler, Jeep, Dodge, Ram, SRT, Mopar and the Pentastar logo are registered trademarks of
     * Chrysler Group LLC. FIAT is a registered trademark of Fiat group Marketing & Corporate
     * Communication S.p.A. used under license by Chrysler Group LLC.
     *********************************************************************************************/
    package com.fca.uconnect.global;

    import java.util.List;

    import com.amazonaws.services.iot.client.AWSIotException;
    import com.amazonaws.services.iot.client.AWSIotMessage;
    import com.amazonaws.services.iot.client.AWSIotMqttClient;
    import com.amazonaws.services.iot.client.AWSIotQos;
    import com.amazonaws.services.iot.client.AWSIotTopic;
    import com.fca.uconnect.global.GlobalUconnectControl.Location;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectAny;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectMessage;
    import com.fca.uconnect.global.GlobalUconnectExtStolenVehAssist.StolenModeChangeRequest;
    import com.fca.uconnect.global.GlobalUconnectExtStolenVehAssist.StolenModeChangeRequest.StolenModeCommand;
    import com.fca.uconnect.global.GlobalUconnectExtStolenVehAssist.StolenModeChangeResponse;
    import com.fca.uconnect.global.GlobalUconnectExtStolenVehAssist.StolenVehicleControlResponse;
    import com.fca.uconnect.global.GlobalUconnectExtStolenVehAssist.StolenVehicleControlResponse.StolenVehControlResponseEnum;
    import com.fca.uconnect.global.GlobalUconnectExtStolenVehAssist.StolenVehicleInfoNotification;
    import com.google.protobuf.ByteString;
    import com.google.protobuf.ExtensionRegistry;

    /**
     * This example class demonstrates how to use the AWS IoT mqtt client to send/receive a Uconnect StolenVehicleAssistance messages to the SDP and wait for a response message.
     * This code is only for reference and is furnished without warranty.....
     *
     * @author FCA Global V2C API Team
     *
     */
    public class TBMExampleForStolenVehAssist {

    	private String clientId; // The clientId is unique to the device and obtained from the client X.509 certificate CN.
    	private ByteString sessionId; // The sessionId is assigned by the SDP to maintain a session independent of connection protocols.
    	private int messageId; // The messageId is a sequential number incremented and assigned to each message sent from the client.
    	private AWSIotMqttClient mqttClient; // The mqtt client object from the AWS IoT client library.
    	private boolean receivedResponse = false; // flag to wait for the response as part of this example.
    	private AWSIotTopic iotTopic; // The Topic object to subscribe for inbound messages.
    	private ExtensionRegistry extRegistry; // Google protocol buffers extension registry instance.
    	private int correlationId = 0;// The correlationId is a sender messageId so that Sender can recognize the message once its received response.
    	private Semaphore semaphore;//The semaphore object is used to wait for a response.
    	List messages ;

    	/**
    	 * Constructor - initialize protocol buffer extension registry for parsing incoming Uconnect Messages.
    	 */
    	public TBMExampleForStolenVehAssist() {
    		extRegistry = ExtensionRegistry.newInstance();
    		extRegistry.add(GlobalUconnectExtStolenVehAssist.stolenModeChangeRequest);
    		extRegistry.add(GlobalUconnectExtStolenVehAssist.stolenModeChangeResponse);
    		extRegistry.add(GlobalUconnectExtStolenVehAssist.stolenVehicleInfoNotification);
    		extRegistry.add(GlobalUconnectExtStolenVehAssist.stolenVehicleControlRequest);
    		extRegistry.add(GlobalUconnectExtStolenVehAssist.stolenVehicleControlResponse);
    		this.semaphore = new Semaphore();
    	}

    	/**
    	 * This method generates a Protocol Buffer Uconnect Message given the required inputs for StolenModeChangeResponse.
    	 *
    	 * @param isStolenModeActive
    	 * @return UconnectMessage Protocol Buffer
    	 */
    	public UconnectMessage getStolenModeChangeRespMsg(boolean isStolenModeActive) {
    		this.messageId++;
    		sessionId = ByteString.copyFrom(new byte[18]);
    		StolenModeChangeResponse stolenModeChgResp = StolenModeChangeResponse.newBuilder()
    			.setIsStolenModeActive(isStolenModeActive)
    			.build();

    		UconnectMessage msg = UconnectMessage.newBuilder()
    			.setTimestamp(System.currentTimeMillis())
    			.setMessageId(messageId)
    			.setCorrelationId(correlationId)
    			.addMessages(UconnectAny.newBuilder().
    			setExtension(GlobalUconnectExtStolenVehAssist.stolenModeChangeResponse, stolenModeChgResp))
    			.build();
    		return msg;
    	}
    	public UconnectMessage getStolenVehNotificationMsg(Location vehicleLocation,boolean isBlockIgnitionActive,
    					boolean isIgnoreAccelerateActive){
    		messageId++;
    		StolenVehicleInfoNotification notifyMsg =StolenVehicleInfoNotification.newBuilder()
    				.setIsBlockIgnitionActive(isBlockIgnitionActive)
    				.setIsIgnoreAccelerateActive(isIgnoreAccelerateActive)
    				.setVehicleLocation(vehicleLocation)
    				.build();
    		UconnectMessage msg = UconnectMessage.newBuilder()
    				.setTimestamp(System.currentTimeMillis())
    				.setMessageId(messageId)
    				.addMessages(UconnectAny.newBuilder().
    				setExtension(GlobalUconnectExtStolenVehAssist.stolenVehicleInfoNotification, notifyMsg))
    				.build();
    			return msg;
    	}
    public UconnectMessage getStolenVehicleControlRespMsg(StolenVehControlResponseEnum respEnum){
    messageId++;
    StolenVehicleControlResponse respMsg =StolenVehicleControlResponse.newBuilder()
    		.setStolenVehControlResponseEnum(respEnum)
    		.build();
    UconnectMessage msg = UconnectMessage.newBuilder()
    		.setTimestamp(System.currentTimeMillis())
    		.setMessageId(messageId)
    		.setCorrelationId(correlationId)
    		.addMessages(UconnectAny.newBuilder().
    		setExtension(GlobalUconnectExtStolenVehAssist.stolenVehicleControlResponse, respMsg))
    		.build();
    	return msg;
    }
    	/**
    	 * This method demonstrates connecting to the AWS IoT mqtt broker and publishing an StolenVehAsist messages to the SVAS topic.
    	 */
    	public void process() {
    		mqttClient = new AWSIotMqttClient("endpoint", clientId, "awsAccessKeyId", "awsSecretAccessKey");
    		try {
    			mqttClient.connect();
    			iotTopic = new AWSIotTopic(clientId+"/SVAS/", AWSIotQos.QOS1) {
    	public void onMessage(AWSIotMessage msg) {
    		try{
    		UconnectMessage msgIn;
    			msgIn = UconnectMessage.parseFrom(msg.getPayload(),extRegistry);
    			correlationId=msgIn.getMessageId();
    	if (msgIn.getMessages(0).hasExtension(GlobalUconnectExtStolenVehAssist.stolenModeChangeRequest)) {
    		semaphore.unlock();// Releasing the lock
    		StolenModeChangeRequest stolenModelChgReqMsg = msgIn.getMessages(0).getExtension(
    				GlobalUconnectExtStolenVehAssist.stolenModeChangeRequest);
    		boolean isStolenModeActive=false;
    	if(stolenModelChgReqMsg.getStolenModeCommand().equals(StolenModeCommand.ENTER))
    			isStolenModeActive=true;
    		UconnectMessage respMsg = getStolenModeChangeRespMsg(isStolenModeActive);
    		sendMessage(respMsg);
    		//For Every interval send Vehicle Notification to SDP with location and Mode
    		int i=1;
    		while(isStolenModeActive){
    			Location vehicleLocation = Location.newBuilder()
    					.setPositionLatitude(42.480201F+(i*0.0001F))
    					.setPositionLongitude(-83.671875F+(i*0.0001F))
    					.build();
    			boolean isBlockIgnitionActive=false;
    			boolean isIgnoreAccelerateActive=false;
    			Thread.sleep(stolenModelChgReqMsg.getLocationUpdateInterval());
    			sendMessage(getStolenVehNotificationMsg(vehicleLocation,
    					isBlockIgnitionActive, isIgnoreAccelerateActive));
    			i++;
    		}
    	}else if(msgIn.getMessages(0).hasExtension(
    			GlobalUconnectExtStolenVehAssist.stolenVehicleControlRequest)){
    		correlationId=msgIn.getMessageId();
    		sendMessage(getStolenVehicleControlRespMsg(StolenVehControlResponseEnum.SUCCESS));
    	}
    	} catch( Exception ex) {
    		ex.printStackTrace();
    		System.out.println("Err processing message: "+ex+", try parsing StolenVehAssistance messages.");
    	}
     }
    };
    			mqttClient.subscribe(iotTopic);
    			this.semaphore.lock();	// lock thread

    		} catch (AWSIotException ex) {
    			System.out.println("Caught AWS Exception "+ex);
    			ex.printStackTrace();
    		}  catch (Exception e) {
    			e.printStackTrace();
    		}
    	}

    	public void sendMessage(UconnectMessage msg) {
    		final byte[] msgOut = msg.toByteArray();
    		new Thread(new Runnable() {
    		    @Override
    		public void run() {
    		try {
    			AWSIotMessage message = new
    					MessagePublisherListener("/SVAS/"+clientId,AWSIotQos.QOS1,msgOut);
    			mqttClient.publish(message);

    		} catch (AWSIotException e) {
    			System.out.println("Caught Exception "+e);
    						e.printStackTrace();
    					}
    			    }
    			}).start();
    		}

    	/**
    	 * Example main to launch example.
    	 *
    	 * @param args
    	 */
    	public static void main(String[] args) {
    		TBMExampleForStolenVehAssist example = new TBMExampleForStolenVehAssist();
    		example.process();
    	}
    }

Here's an example of how Service Connects to AWS IOT MQTT for SVAS topics and process Stolen Vehicle Assistance messages.

Example Code (SDP):

    package com.fca.uconnect.global;
    import com.amazonaws.services.iot.client.AWSIotException;
    import com.amazonaws.services.iot.client.AWSIotMessage;
    import com.amazonaws.services.iot.client.AWSIotMqttClient;
    import com.amazonaws.services.iot.client.AWSIotQos;
    import com.amazonaws.services.iot.client.AWSIotTopic;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectAny;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectMessage;
    import com.fca.uconnect.global.GlobalUconnectExtStolenVehAssist.StolenModeChangeRequest;
    import com.fca.uconnect.global.GlobalUconnectExtStolenVehAssist.StolenModeChangeRequest.StolenModeCommand;
    import com.fca.uconnect.global.GlobalUconnectExtStolenVehAssist.StolenVehicleControlRequest;
    import com.google.protobuf.ByteString;
    import com.google.protobuf.ExtensionRegistry;

    public class SDPExampleForStolenVehAssist {
    private String clientId; // The clientId is unique to the device and obtained from the client X.509 certificate CN.
    private ByteString sessionId; // The sessionId is assigned by the SDP to maintain a session independent of connection protocols.
    private int messageId=10; // The messageId is a sequential number incremented and assigned to each message sent from the client.
    private AWSIotMqttClient mqttClient; // The mqtt client object from the AWS IoT client library.
    private AWSIotTopic iotTopic; // The Topic object to subscribe for inbound messages.
    private ExtensionRegistry extRegistry; // Google protocol buffers extension registry instance.
    private int stolenVehicleControlmessageId;// This is to store message Id that sent with stolenVehicleControlRequest.
    private boolean vehControlReqSent=false;//This is to check whether SDP received Vehicle Notification.

    public SDPExampleForStolenVehAssist() {
    	extRegistry = ExtensionRegistry.newInstance();
    	extRegistry.add(GlobalUconnectExtStolenVehAssist.stolenModeChangeRequest);
    	extRegistry.add(GlobalUconnectExtStolenVehAssist.stolenModeChangeResponse);
    	extRegistry.add(GlobalUconnectExtStolenVehAssist.stolenVehicleInfoNotification);
    	extRegistry.add(GlobalUconnectExtStolenVehAssist.stolenVehicleControlResponse);
    	extRegistry.add(GlobalUconnectExtStolenVehAssist.stolenVehicleControlRequest);
    }

    public UconnectMessage getStolenVehicleControlReqMsg(boolean isIgnoreAccelerate,boolean isBlockIgnition){
    	messageId++;
    	stolenVehicleControlmessageId =messageId;
    	StolenVehicleControlRequest sControlReqMsg = StolenVehicleControlRequest.newBuilder()
    			.setIsIgnoreAccelerate(true)
    			.setIsBlockIgnition(true)
    			.build();
    	UconnectMessage msg = UconnectMessage.newBuilder()
    		.setTimestamp(System.currentTimeMillis())

    		.setMessageId(messageId)
    		.addMessages(UconnectAny.newBuilder().
    		 setExtension(GlobalUconnectExtStolenVehAssist.stolenVehicleControlRequest,sControlReqMsg))
    		.build();
    	return msg;

    }
    public UconnectMessage getStolenModeChgReqMsg(boolean isActiveWhenKeyOff,int locationUpdateInterval,
    		StolenModeCommand stolenModeCommand,int stolenModeDuration) {
    	messageId++;
    	StolenModeChangeRequest sreq = StolenModeChangeRequest.newBuilder()
    			.setIsActiveWhenKeyOff(isActiveWhenKeyOff)
    			.setLocationUpdateInterval(locationUpdateInterval)
    			.setStolenModeCommand(stolenModeCommand)
    			.setStolenModeDuration(stolenModeDuration)
    			.build();
    	UconnectMessage msg = UconnectMessage.newBuilder()
    		.setTimestamp(System.currentTimeMillis())

    		.setMessageId(messageId)
    		.addMessages(UconnectAny.newBuilder().
    		 setExtension(GlobalUconnectExtStolenVehAssist.stolenModeChangeRequest,sreq))
    		.build();

    	return msg;
    }

    public void process() {
    	mqttClient = new AWSIotMqttClient("endpoint", clientId, "awsAccessKeyId", "awsSecretAccessKey");

    try {
    mqttClient.connect();
     iotTopic = new AWSIotTopic("/SVAS/#",AWSIotQos.QOS1){
    	public void onMessage(AWSIotMessage msg) {
    try {

    	UconnectMessage	msgIn = UconnectMessage.parseFrom(msg.getPayload(),extRegistry);
    	int msgId = msgIn.getMessageId();
    		if(msgIn.getMessages(0).hasExtension(
    		  GlobalUconnectExtStolenVehAssist.stolenVehicleInfoNotification)){
    		//Receive Vehicle Information from TBM

    		if(!vehControlReqSent){
    			vehControlReqSent=true;
    			try {
    				Thread.sleep(2000);
    			} catch (InterruptedException e) {
    			}
    			sendMessage(getStolenVehicleControlReqMsg(true,true));//send Stolen Vehicle control Request
    		}
    	}else if (msgIn.getMessages(0).hasExtension(
    			GlobalUconnectExtStolenVehAssist.stolenModeChangeResponse) &&
    			msgIn.getCorrelationId() ==messageId){
    		//receive response from TBM
    	}else if (msgIn.getMessages(0).hasExtension(
    			GlobalUconnectExtStolenVehAssist.stolenVehicleControlResponse) &&
    			msgIn.getCorrelationId()==stolenVehicleControlmessageId){
    		//Receive Stolen VehicleControl Response
    	}

    } catch( Exception ex) {
    	ex.printStackTrace();
    	System.out.println("Err processing message: "+ex+", try parsing Stolen Vehicle Assistance.");

    }
    }
    };

    sendMessage(getStolenModeChgReqMsg(false, 100000, StolenModeCommand.ENTER, 1000000));
    mqttClient.subscribe(iotTopic);

    } catch (AWSIotException e) {
    	System.out.println("Caught Exception "+e);
    	e.printStackTrace();
    }
    }

    public void sendMessage(UconnectMessage msg) {
    final byte[] msgOut = msg.toByteArray();
    new Thread(new Runnable() {
        @Override
    public void run() {
    try {
    	AWSIotMessage message = new
    			MessagePublisherListener(clientId+"/SVAS/",AWSIotQos.QOS1,msgOut);
    	mqttClient.publish(message);

    } catch (AWSIotException e) {
    	System.out.println("Caught Exception "+e);
    				e.printStackTrace();
    			}
    	    }

    	}).start();
    }
    public static void main(String[] args) {
    	SDPExampleForStolenVehAssist m = new SDPExampleForStolenVehAssist();
    	m.process();
    }
    }

The example code demonstrates how to connect with AWS IoT for publishing and subscribing to the SVAS topic.

Download Client Example Code here

Download Service Example Code here