This is the 2.6 approved release of the Global API distributed to Global suppliers. While it is considered "production" ready and has been gate approved, it is being marked pre-release because integration development is in process. 

# API Versions in this release

| API/Proto file | Description | Version | Version Date |
|--------------------------------------------------|-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------|---------|--------------|
| Global_Uconnect_Control.proto | Main message proto file. Contains the Uconnect message wrapper, Keep Alive and Ack message definitions | 1.16 | 04/23/2018 |
|  |  |  |  | 
| Global_Uconnect_Device.proto | Used for common device information messages | 1.3 | 04/2/2018 |
| Global_Uconnect_DRM.proto | Used for Common DRM Messages | 1.1 | 11/2/2017 |
| Global_Uconnect_GNSS.proto | The proto is utilized for Destination,Address,POI and location used in other Protobuff | 1.4 | 04/30/2018 |
| Global_Uconnect_VehicleInfo.proto | The common proto is utilized for VehicleInfo and VehicleStatus | 1.1 | 9/20/2017 |
| Global_Uconnect_Ext_Activation.proto | This API supports the In-Vehicle Activation process by submitting a request to the SDP when the vehicle is first activated by the customer. | 1.4 | 11/2/2017 |
| Global_Uconnect_Ext_AOTA.proto | This API is to notify the AOTA client of an update.  The AOTA client will manage downloading the update most likely through a different channel (https). | 1.2 | 11/2/2017 |
| Global_Uconnect_Ext_Auth.proto | This API supports the client sending both User and Device identifier and credentials to the SDP.  For Users the SDP replies with the login results.  Upon successful login, the SDP will push a provisioning message to the client with personal account settings associated with the provided user identity.The API is also to support a personal account.  The SDP must know the identity of the user prior to delivering personal account data to the vehicle. | 1.6 | 03/12/2018 |
| Global_Uconnect_Ext_CommCheck.proto | The Proto is to utilize the common Authorization and Comm Check Messages, often referred to as bootstrap. | 1 | 12/112017 |
| Global_Uconnect_Ext_Ecall.proto | This is to define Emergency Call.When ECall is triggered, Phone call will be dialed out to the call center.The operator may expect to see the vehicle related information when the phone call is connected. Client  gathers vehicle information and send it out.Before the phone call is connected, the user also has the chance to cancel the Ecall. | 1.8 | 11/2/2017 |
| Global_Uconnect_FOTA.proto | This API notify the FOTA client of an update.  The FOTA client will manage downloading the update most likely through a different channel (https). | 1.2 | 11/2/2017 |
| Global_Uconnect_Ext_IVH.proto | IVH-In Vehicle Help,This API is to notify when new Help Content is available for download.  The IVH client will manage downloading the update most likely through a different channel (https). | 1.2 | 11/2/2017 |
| Global_Uconnect_Ext_PC.proto | This API enables the SDP to configure the TBM for Parental Control data collection and notification.The feature supports notifying the vehicle owner with alerts for geofencing, curfew, speed, valet, and similar events. | 1.4 | 11/2/2017 |
| Global_Uconnect_Ext_PerformancePages.proto | Uploads Track Data | 1.1 | 11/2/2017 |
| Global_Uconnect_Ext_PHEV.proto | PHEV regulatory data for apac | 1.2 | 11/2/2017 |
| Global_Uconnect_Ext_POISearch.proto | This API supports the POI Search Requests. | 1.2 | 11/2/2017 |
| Global_Uconnect_Ext_Provision.proto | The Provisioning API supports the client requesting or the SDP pushing the vehicle provisioning information to the client.The interface includes the read-only configuration data consumed by the client.  The Vehicle Data Sync interface supports the data elements which can be modified in the vehicle and synchronized with the cloud. | 1.16 | 11/2/2017 |
| Global_Uconnect_Ext_RemoteOp.proto | This API supports the Remote Operations. | 1.11 | 04/23/2018 |
| Global_Uconnect_Ext_RoadSideAssist.proto | This API is to define Road Side Assistance. When Bluetooth is triggered, Phone call will be dialed out to the call center.The operator may expect to see the vehicle related information when the phone call is connected. Client  gathers vehicle information and send it out. | 1.4 | 11/2/2017 |
| Global_Uconnect_Ext_SendAndGo.proto | This API is to push some destinations to the vehicle, the SDP shall send the destinations data to the TBM when the TBM is connected.TBM will save the destination. | 1.3 | 11/2/2017 |
| Global_Uconnect_Ext_Signature.proto | This is for validation and protection for all the messages that are stored in TU. | 1.3 | 11/2/2017 |
| Global_Uconnect_Ext_SQDF.proto | This message is to define SQDF | 1.9 | 04/25/2018 |
| Global_Uconnect_Ext_StolenVehiAssist.proto | This API is to assist the User in case of Vehicle is Stolen, and User  alerts the SDP (by means the call center)  then the SDP sends info to the client.When the vehicle is stolen, the SDP side can send out request to the User, asking the TBM to enter into the SVA mode.The SDP shall also send a cancel request asking the TBM to exit the SVA mode.The TBM shall respond with a message with related vehicle information required by the SVA service. | 1.2 | 11/2/2017 |
| Global_Uconnect_Ext_TheftAlarmNotify.proto | This API is to notify the User in case of steal or tamper with car.When Theft alarm is detected Client sends Information to SDP to alert the User. | 1.4 | 04/30/2018 |
| Global_Uconnect_Ext_VehicelDataAcquisition.proto | The messages in Global_Uconnect_Ext_VehDataAcquisition.proto define a flexible mechanism for collecting data from vehicles. | 1.5 | 11/2/2017 |
| Global_Uconnect_Ext_VehicleFinder.proto | This API is to find the location of the vehicle on demand | 1.3 | 11/2/2017 |
| Global_Uconnect_Ext_VehicleMessenger.proto | This API enables the SDP to send messages to HU , the HU messages that should be displayed to the operator of the vehicle, and the HU to notify the SDP when messages were displayed and the operator's response. | 1.2 | 11/2/2017 |
| Global_Uconnect_Ext_VehicleSync.proto | This API is to publish configuration changes to the vehicle. | 1.14 | 11/30/2017 |
| Global_Uconnect_Ext_WIFIHostspot.proto | This proto is for getting WIFI Data Status and sending Push if there is low Data. | 1.1 | 11/2/2017 |
| Global_Uconnect_Ext_ConnectedPages.proto | This proto is for Uploading Eco and OffroadPages Info. | 1.1 | 03/12/2018 |
| Certificate Management |  | 1 | 3/8/2017 |