# FCA Global Vehicle-to-Cloud API Project Page  

[Global V2C API Specifications](https://collab.intra.fcagroup.com/sites/GTBM/default.aspx?RootFolder=%2Fsites%2FGTBM%2FShared%20Documents%2FSFS_Global_FINAL%2FSFS_repository&FolderCTID=0x0120001D562954E30E0744A2454AA6A8A6DD61&View=%7B69557297-FE2C-46D7-8109-BE5123F2A896%7D)  
  
[Developer Access or Repository Clone](https://shc004gitp01.shdc.chrysler.com/Uconnect/Global-API)  


The FCA Uconnect Global API’s define a standard data communication protocol for the Telematics Unit in the vehicle to interface with the cloud based Service Delivery Platform (SDP). The in-vehicle unit consists of either a Telematics Box Module (TBM) or Head Unit (HU), while the SDP can be hosted in any one of many cloud based infrastructures including Amazon Web Services (AWS).

API are generally mapped to a specific service (e.g. IVH In Vehicle Help), therefore relative documentation for a service should be carefully descriptor in each API.

The primary objective of this API is to create interoperability between the FCA regions including APAC, EMEA, LATAM, and NAFTA which with proper adoption will result in efficiency improvements and cost reductions as platforms become more global. Additionally, the API will improve the FCA Connected Vehicle Platform design for performance, scalability, flexibility, security, maintainability, and cost effectiveness.

Vehicle-to-Cloud APi will represent the reference schema for the Onboard implementation and the SDP implementation, thus closing the bridge between the vehicle and the cloud platform.
SFS, or Service Feature Specifications, will be a more readable form of the V2C API; the source-of-truth will be implemented in the Github APIs Specs.

This is the actual reference schema:  
![Vehicle Schema](https://gsdp.github.intra.fcagroup.com/GSDP-V2C/global-api/blob/master/Vehicle%20reference%20schema.PNG)


global-api/fca_global_api-master/documents/API/images/Vehicle reference schema.PNG

This is the V2C API schema:
![Vehicle Schema](https://shc004gitp01.shdc.chrysler.com/uconnect-ict/global-api/blob/master/v2cContext.png)

The API is based on industry best-practices for the Internet of Things (IoT) including the use of the secure MQTT and HTTP communication protocols. The need to minimize costly wireless network traffic has also lead to the use of Protocol Buffers for efficiently formatting the data into messages between the client (TBM or HU) and the services (SDP).

## DRM Usage

The DRM file (also known as `drm.properties`/`drm.jar`/`drm.apk`) will always be included as a `base64` encoded binary data in the `drmFile` field of the protobuf.

For `JVM` (Java Virtual Machine) based systems, the DRM signature is already enclosed in the `JAR` file and it will not need the `DRMSignature` message in the `DRM` protobuf.

For `Android` based systems, the DRM signature is already enclosed in the `APK` file and it will not need the `DRMSignature` message in the `DRM` protobuf.

All the other ECUs not described above, will follow the `GENERIC` content type strategy:
* the DRM file will be the `drm.properties` (`base64` encoded).
* the DRM signature will be enclosed in the `DRMSignature` message in the `DRM` protobuf.
* the DRM file as received will be stored in a ECU supported format

## File types for the DRM 

| ECU Name | Supplier        | Content Type | Notes    |
| -------- | --------------- | ------------ | -------- |
| VP2R     | Aptiv/Delphi    | JVM          | drm.jar  |
| VP2R     | Continental     | GENERIC      | protobuf |
| VP4R     | Panasonic       | JVM          | drm.jar  |
| J6       | HARMAN          | JVM          | drm.jar  |
| G2.5     | Magneti Marelli | GENERIC      | protobuf |
| R1L      | Melco           | APK          | drm.apk  |
| R1H      | HARMAN          | APK          | drm.apk  |
| TBM2.0   | Magneti Marelli | GENERIC      | protobuf |


## System Level Error Codes

 For App Level Error codes refer to the feature proto file and the application documentation.
 

| Code | Error | Description |
|------|-------|-------------|
| 200 | OK | OK/Success Message |
| 400 | Bad Request | If the GSDP cannot process the message from the mqtt topic (Protobuf fails parsing, etc.) |
| 401 | Unauthorized | If the clientId associated with the connection is not authorized to send a message to the mqtt topic |
| 403 | Forbidden | If the message was received on a forbidden topic |
| 404 | Not Found | If the message was sent to an unknown topic |
| 408 | Request Timeout | If the logic warrants, and a timeout event occurs |
| 413 | Payload too large | If the message size exceeds a defined threshold (a threshold is required to protect against sending malicious messages to the protobuf parser) |
| 500 | Internal Server Error | If on the server an error is encountered processing a message |
| 501 | Not Implemented | If the service is not implemented to handle messages on a known topic |
| 503 | Service Unavailable | If the service is unavailable for handling messages on a known topic |

## Using Vehicle Data Acquisition Publish API without ADA 

The initial release of TBM software will not make use of the ADA enabler application. This impacts applications including Traffic Probes, UBI and Remote Vehicle Status. These features are targeted to use the ADA and the Global API Vehicle Data Acquisition Publish (**VDAP**) API was designed to work with the ADA.  

Features can still take advantage of the open design of VDAP API without ADA, there is a particular consideration that must be addressed during implementation where the ADA is not  being used.  

The VDAP API is design to publish to a single topic *topic/ADA/${iot:ClientId}* and was defined to make use of a message body element *policySubscriptionId: "-\0274\302]\325\324 \354K"* to identify which policy's data the ADA is publishing. In this scenerio, a feature to policy mapping is necessary in the back end.  

Without the ADA, it shall be necessary that the same field is employed to identify which application is publishing the message, this is a byte field as defined and should be consumed as such so that switching to policy based subscriptions when the ADA is deployed is seamless. 
 
## Offroad Pages Signals
|    | PNet Message.Signal               | LID                              | CANBus             | Bus CycleRate (ms) | API CycleRate (ms) |   | Data calculation type (once,on change,min,average,max) | Data calculation interval (sec) = Y                | Global snapshot sending time period to GSDP (min) = X |    |                 |                 | KONA Sensor Name                                                                              | Context Type | Description                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               | State                                                                                      | Is Writable | Is Available | CAN Signal            | Max Buffer    | Number of Channels | Channel Name                     | SensorType    | Data Type   | Min Abs Range | Max Abs Range | Resolution | Unit                                     |
|----|-----------------------------------|----------------------------------|--------------------|--------------------|--------------------|---|--------------------------------------------------------|----------------------------------------------------|-------------------------------------------------------|----|-----------------|-----------------|-----------------------------------------------------------------------------------------------|--------------| |--------------------------------------------------------------------------------------------|-------------|--------------|-----------------------|---------------|--------------------|----------------------------------|---------------|-------------|---------------|---------------|------------|------------------------------------------|
| 7  | GW_C_I_11.ACT_R_DIF_TRQ           | ActualRearDifferentialTorqueLock | BH                 | 200                | 200                |   | min,average,max                                        | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      | WK | VF737           |                 | ActualRearDifferentialTorqueLockThe range of the ACT_R_DIF_TRQ signal values is 0 to 2540 Nm. | device       | ActualRearDifferentialTorqueLock sensor. It has one channel, which tells the Actual rear differential torque lock value. This sensor cannot be switched off and is always available.The range of the ACT_R_DIF_TRQ signal values is 0 to 2540 Nm.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         |                                                                                            | FALSE       | TRUE         | ACT_R_DIF_TRQ         | 256           | 1                  | ActualRearDifferentialTorqueLock |               | TYPE_INT    | 0             | 2540          | 10         |                                          |
| 8  | GW_C_I_11.ASCM_Stat               | AirSuspensionStatus              | BH                 | 200                | 200                |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | AirSuspensionStatus                                                                           | device       | AirSuspensionStatus sensor. It has one channel, which tells the Air suspension status. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        |                                                                                            | FALSE       | TRUE         | ASCM_Stat             | 256           | 1                  | AirSuspensionStatus              |               | TYPE_INT    | 0             | 15            | 1          |                                          |
| 51 | ASCM_2.ASCM_Srv                   | ServiceAirSuspension             | C                  | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | ASCM_Srv                                                                                      | device       | Service air suspension                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    |                                                                                            | FALSE       | TRUE         | ASCM_Srv              | 256           | 1                  | ASCM_Srv                         |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 52 | ASCM_2.ASCM_SysFail               | ASCM_SysFail                     | C                  | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | ASCM_SysFail                                                                                  | device       | Loss of function - system fault                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | ASCM_SysFail          | 256           | 1                  | ASCM_SysFail                     |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 76 | DTCM_B1.AxleLckrEVICDisplay       | AxleLckrEVICDisplay              | C                  | 1000               | 1000               |   | Never                                                  |                                                    | Never                                                 | JL |                 |                 | AxleLckrEVICDisplay                                                                           | vehicle      | Axle locker HMI display request                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | AxleLckrEVICDisplay   | 256           | 1                  | AxleLckrEVICDisplay              | state         | TYPE_INT    | 0             | 15            | 1          |                                          |
| 72 | DTCM_B1.AxleLckrSts               | AxleLckrSts                      | C                  | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      | JL |                 |                 | AxleLckrSts                                                                                   | vehicle      | Axle locker status: VC_AxleLockerPrsnt = REAR 0=Unlocked(Rear Axle is Unlocked)1=RR_LKD(Rear Axle is Locked) 3=SNAVC_AxleLockerPrsnt = FTRR 0=Unlocked(Front and Rear Axle is Unlocked)1=RR_LKD(Front is Unlocked and Rear Axle is Locked) 2=FR_RR_LKD(Front and Rear Axle Locked) 3=SNA                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  |                                                                                            | FALSE       | TRUE         | AxleLckrSts           | 256           | 1                  | AxleLckrSts                      | state         | TYPE_INT    | 0             | 3             | 1          |                                          |
| 22 | CBC_I3.BATT_VOLT                  | BatteryVoltage                   | BH                 | 200                | 200                |   | average                                                | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF008           |                 | Battery                                                                                       | vehicle      | Battery voltage sensor is a range based component. It has one channel, which returns the battery voltage level. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               |                                                                                            | FALSE       | TRUE         | BATT_VOLT             | 256           | 1                  | Battery                          | range         | TYPE_DOUBLE | 5             | 18            | 0.1        | Volts                                    |
| 35 | PN14_STAT.Batt_ST_Crit            |                                  | BH                 | 500                | 500                |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | BatteryLampStatus                                                                             | device       | Battery Lamp Status                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                       |                                                                                            | FALSE       | TRUE         | Batt_ST_Crit          | 256           | 1                  | Batt_ST_Crit                     |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 79 | TCM_A7.CurrentGearForDisplay      | CurrentGearForDisplay            | C                  | 20                 | 200                |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      | JL | VF446           |                 | CurrentGearForDisplay                                                                         | vehicle      | Current Gear for display                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  |                                                                                            | FALSE       | TRUE         | CurrentGearForDisplay | 256           | 1                  | CurrentGearForDisplay            | state         | TYPE_INT    | 0             | 15            | 1          |                                          |
| 49 | ENG_CFG.DISPLACEMENT              | DISPLACEMENT                     | C                  | 100                | 1000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 | Displacement                                                                                  | device       | Displacement sensor. It has one channel which tells Engine displacement. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      |                                                                                            | FALSE       | TRUE         | DISPLACEMENT          | 256           | 1                  | Displacement                     |               | TYPE_DOUBLE | 0             | 25            | 0.1        | liters                                   |
| 29 | GW_LIN_C_I2.DistanceUnit          | DistanceUnit                     | BH                 | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | DistanceUnit                                                                                  | device       | DistanceUnit sensor. It has one channel which tells you the Distance (odometer) units. Miles = [1]. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | DistanceUnit          | 256           | 1                  | DistanceUnit                     |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 81 | EcuCfg4.EC_Cluster1A              | EC_Cluster1A                     | C                  | 2000               | 2000               |   | Never                                                  |                                                    | Never                                                 | JL |                 |                 | EC_Cluster1A                                                                                  | vehicle      | Instrument cluster ecu configuration 1A                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   |                                                                                            | FALSE       | TRUE         | EC_Cluster1A          | 256           | 1                  | EC_Cluster1A                     | state         | TYPE_INT    | 0             | 3             | 1          |                                          |
| 23 | GW_C_I2.EngCoolTemp               | EngineCoolant                    | BH                 | 1000               | 1000               |   | min,average,max                                        | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF016           |                 | EngineCoolant                                                                                 | vehicle      | EngineCoolant sensor is a range based component. It has one channel, which returns the Engine Coolant temperature. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            |                                                                                            | FALSE       | TRUE         | EngCoolTemp           | 256           | 1                  | EngineCoolant                    | range         | TYPE_INT    | -40           | 214           | 1          | °C                                       |
| 62 | ECM_INDICATORS.OIL_TEMP_IND_RQ    | EngineOilOverTemp                | C                  | 100                | 200                |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | EngineOilOverTemp                                                                             | device       | EngineOilOverTemp sensor. It has one channel, which returns the EngineOilOverTemp value.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  |                                                                                            | FALSE       | TRUE         | OIL_TEMP_IND_RQ       | 256           | 1                  | EngineOilOverTemp                |               | TYPE_INT    | 0             | 3             | 1          |                                          |
| 47 | ECM_INDICATORS.EngOilTemp         | OilTemp                          | C                  | 100                | 100                |   | min,average,max                                        | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF671           |                 | EngineOilTemp                                                                                 | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | EngOilTemp            | 256           | 1                  | EngOilTemp                       |               | TYPE_INT    | 0             | 6             | 1          |                                          |
| 65 | GW_C1.EngRPM                      | EngineRPM                        | BH                 | 100                | 200                |   | min,average,max                                        | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | EngineRPM                                                                                     | vehicle      | EngRPM sensor is a range based component. It has one channel, which returns the Engine RPM value. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             |                                                                                            | FALSE       | TRUE         | EngRPM                | 256           | 1                  | EngineRPM                        | range         | TYPE_INT    | 0             | 65535         | 1          | rpm                                      |
| 9  | GW_C_I_11.FL_Lvl                  | FrontLeftLevel                   | BH                 | 200                | 200                |   | min,max                                                | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | FrontLeftLevelNOTE: The range of the suspension level signals values is -100 to 155 mm        | device       | FrontLeftLevel sensor. It has one channel, which tells the Front left level. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  |                                                                                            | FALSE       | TRUE         | FL_Lvl                | 256           | 1                  | FrontLeftLevel                   |               | TYPE_INT    | -100          | 155           | 1          |                                          |
| 10 | GW_C_I_11.FR_Lvl                  | FrontRightLevel                  | BH                 | 200                | 200                |   | min,max                                                | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | FrontRightLevelNOTE: The range of the suspension level signals values is -100 to 155 mm       | device       | FrontRightLevel sensor. It has one channel, which tells the Front right level. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                |                                                                                            | FALSE       | TRUE         | FR_Lvl                | 256           | 1                  | FrontRightLevel                  |               | TYPE_INT    | -100          | 155           | 1          |                                          |
| 74 | DTCM_B1.Ft_RrAxleLkIndRq          | Ft_RrAxleLkIndRq                 | C                  | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      | JL |                 |                 | Ft_RrAxleLkIndRq                                                                              | vehicle      | Front and Rear axle lock indicator request                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                |                                                                                            | FALSE       | TRUE         | Ft_RrAxleLkIndRq      | 256           | 1                  | Ft_RrAxleLkIndRq                 | state         | TYPE_INT    | 0             | 3             | 1          |                                          |
| 24 | GW_C_I2.FUEL_TYPE                 | FuelType                         | BH                 | 1000               | 1000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 | FuelType                                                                                      | device       | FUEL_TYPE sensor. It has one channel, which returns the Fule type status value.0=UNLEADED1=Diesel3=Flex Fuel                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              |                                                                                            | FALSE       | TRUE         | FUEL_TYPE             | 256           | 1                  | FUEL_TYPE                        |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 25 | GW_C_I3.LANG_C                    | LanguageSelection                | BH                 | 500                | 500                |   | Once (At HU app launch)                                | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | getCurrentLocale  (Unkonwn)LanguageSelection                                                  | device       | This signal is used to give information about the Language selected                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                       |                                                                                            | FALSE       | TRUE         | LANG                  | 256           | 1                  | LANG                             |               | TYPE_INT    | 0             | 255           | 1          |                                          |
| 21 | CBC_I2.GlobDrvMdSts               | GlobDrvMdSts                     | BH                 | 500                | 500                |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | GlobDrvMdSts                                                                                  | vehicle      | Global drive mode status                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  |                                                                                            | FALSE       | TRUE         | GlobDrvMdSts          | 256           | 1                  | GlobDrvMdSts                     | state         | TYPE_INT    | 0             | 32            | 1          |                                          |
| 17 | VehCfg1.VC_HDC_Prsnt              | HillDescent                      | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    | VF395           |                 | HillDescent                                                                                   | device       | If HDC is Present on Vehicle.  HillDescent sensor . It has one channel, which tells if the Hill descent feature is present[1]. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                |                                                                                            | FALSE       | TRUE         | VC_HDC_Prsnt          | 256           | 1                  | HillDescent                      |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 2  | GW_C_I2.HILL_DES_STAT             | HillDescentStatus                | BH                 | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF395           |                 | HillDescentStatus                                                                             | device       | HillDescentStatus sensor. It has one channel, which tells the Hill descent feature status. This sensor cannot be switched off and is always available.0=HDC_UNAVL1=HDC_ACT2=HDC_AVL3=HDC_THRML_DEACT                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      |                                                                                            | FALSE       | TRUE         | HILL_DES_STAT         | 256           | 1                  | HillDescentStatus                |               | TYPE_INT    | 0             | 3             | 1          |                                          |
| 6  | GW_C_I6.LRWS_ST                   | LRWS_ST                          | BH                 | 100                | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF737           |                 | LRWS_ST                                                                                       | device       | 0=OK1=INI(Not Initialized)2=ERR(Fault)3=ERR_INI(Fault and Not Initialized)                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                |                                                                                            | FALSE       | TRUE         | LRWS_ST               | 256           | 1                  | LRWS_ST                          |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 44 | SCCM_STW_ANGL_STAT.LRW_PLRTY      | LRW_PLRTY                        | C                  | 10                 | 1000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    | VF737           |                 | LRW_PLRTY                                                                                     | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | LRW_PLRTY             | 256           | 1                  | LRW_PLRTY                        |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 5  | GW_C_I6.LRW                       | SteeringWheelAngle               | BH                 | 100                | 100                |   | min,max                                                | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF737           |                 | SteeringWheelAngle                                                                            |              | The range of the LRW and signal values is -2048 to 2047 degrees.WK(ONLY)+569 Shall represent front wheels pointing to Full Left-569 Shall represent front wheels Pointing to Full RightJL(ONLY)2.8.9.14 (JL Only) LRW_PLRTY(Kona) = [0]  and VC_BODY_STYLE(Kona)= Station Wagon , then +645.5 Shall represent front wheels pointing to Full Left2.8.9.15 (JL Only) LRW_PLRTY(Kona) = [0]  and VC_BODY_STYLE(Kona)= Station Wagon , then -645.5 Shall represent front wheels Pointing to Full Right2.8.9.16 (JL Only) LRW_PLRTY(Kona) = [0]  and VC_BODY_STYLE(Kona)= Hatch Back, then +568 Shall represent front wheels pointing to Full Left2.8.9.17 (JL Only) LRW_PLRTY(Kona) = [0]  and VC_BODY_STYLE(Kona)= Hatch Back, then -568 Shall represent front wheels Pointing to Full Right | SteeringWheelAngle sensor. It has one channel, which returns the SteeringWheelAngle value. |             | FALSE        | LRW                   | 256           | 1                  | SteeringWheelAngle               |               | TYPE_DOUBLE | -2048         | 2047          | 0.5        | Degrees                                  |
| 20 | NET_CFG_PT.NET_CFG_STAT_PT        | NET_CFG_STAT_PT                  | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 | NET_CFG_STAT_PT                                                                               | vehicle      | Backup for network configuration status                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   | 0,1,2,3                                                                                    | FALSE       | TRUE         | NET_CFG_STAT_PT       | 256           | 1                  | NET_CFG_STAT_PT                  | state         | TYPE_INT    | 0             | 3             | 1          |                                          |
| 69 | NET_CFG_PT.NetCfg_ASBS            | NetCfg_ASBS                      | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     | JL |                 |                 | NetCfg_ASBS                                                                                   | vehicle      | Automatic Sway Bar System Module (Present = 1, Not Present = 0)                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | NetCfg_ASBS           | 256           | 1                  | NetCfg_ASBS                      | state         | TYPE_INT    | 0             | 1             | 1          |                                          |
| 63 | ECM_INDICATORS.OIL_IND_LMP_FLSH   | OIL_IND_LMP_FLSH                 | C                  | 100                | 200                |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | OIL_IND_LMP_FLSH                                                                              | vehicle      | Oil indicator lamp flash (for in plant use)                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               |                                                                                            | FALSE       | TRUE         | OIL_IND_LMP_FLSH      | 256           | 1                  | OIL_IND_LMP_FLSH                 | state         | TYPE_INT    | 0             | 1             | 1          |                                          |
| 48 | ECM_INDICATORS.OIL_PRESS          | OilPressure                      | C                  | 100                | 100                |   | min,average,max                                        | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF691           |                 | OilPressure                                                                                   | vehicle      | OilPressure sensor is a range based component. It has one channel, which returns the OilPressure value.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   |                                                                                            | FALSE       | TRUE         | OIL_PRESS             | 256           | 1                  | OilPressure                      | range         | TYPE_INT    | 0             | 1016          | 4          | kPaG                                     |
| 36 | VehCfg1.VC_PP_Prsnt               | VC_PP_Prsnt                      | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 | PerformancePagesPresent                                                                       | device       | PerformancePagesPresent sensor. It has one channel, which tells if the Performance Pages is Present. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                          |                                                                                            | FALSE       | TRUE         | VC_PP_Prsnt           | 256           | 1                  | PerformancePagesPresent          |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 27 | GW_C_I_10.Pitch_Angle             | PitchAngle                       | BH                 | 100                | 100                |   | min,average,max                                        | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF683           |                 | PitchAngle                                                                                    | device       | PitchAngle sensor. It has one channel, which tells the Pitch angle. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | Pitch_Angle           | 256           | 1                  | PitchAngle                       |               | TYPE_INT    | -90           | 90            | 1          |                                          |
| 30 | GW_LIN_C_I2.PressureUnit          | PressureUnit                     | BH                 | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | PressureUnit                                                                                  | device       | PressureUnit sensor. It has one channel which tells you the Pressure units. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   |                                                                                            | FALSE       | TRUE         | PressureUnit          | 256           | 1                  | PressureUnit                     |               | TYPE_INT    | 0             | 2             | 1          |                                          |
| 3  | GW_C_I3.PRNDL_DISP                | PRNDL_Display_Request            | BH                 | 500                | 500                |   | Never                                                  |                                                    | Never                                                 |    |                 |                 | PRNDL_Display_Request                                                                         | device       | PRNDL_Display_Request sensor. It has one channel, which tells the PRNDL display request. This sensor cannot be switched off and is always available.0=LVR_P1=LVR_R2=LVR_N4=LVR_D5=NOT_R7=SNA                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              |                                                                                            | FALSE       | TRUE         | PRNDL_DISP            | 256           | 1                  | PRNDL_Display_Request            |               | TYPE_INT    | 32            | 255           | 1          |                                          |
| 11 | GW_C_I_11.RL_Lvl                  | RearLeftLevel                    | BH                 | 200                | 200                |   | min,max                                                | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | RearLeftLevelNOTE: The range of the suspension level signals values is -100 to 155 mm         | device       | RearLeftLevel sensor. It has one channel, which tells the Rear left level. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    |                                                                                            | FALSE       | TRUE         | RL_Lvl                | 256           | 1                  | RearLeftLevel                    |               | TYPE_INT    | -100          | 155           | 1          |                                          |
| 12 | GW_C_I_11.RR_Lvl                  | RearRightLevel                   | BH                 | 200                | 200                |   | min,max                                                | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | RearRightLevelNOTE: The range of the suspension level signals values is -100 to 155 mm        | device       | RearRightLevel sensor. It has one channel, which tells the Rear right level. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  |                                                                                            | FALSE       | TRUE         | RR_Lvl                | 256           | 1                  | RearRightLevel                   |               | TYPE_INT    | -100          | 155           | 1          |                                          |
| 28 | GW_C_I_10.Roll_Angle              | RollAngle                        | BH                 | 100                | 100                |   | min,average,max                                        | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF683           |                 | RollAngle                                                                                     | device       | RollAngle sensor. It has one channel, which tells the Roll angle. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             |                                                                                            | FALSE       | TRUE         | Roll_Angle            | 256           | 1                  | RollAngle                        |               | TYPE_INT    | -90           | 90            | 1          |                                          |
| 75 | DTCM_B1.RrAxleLkIndRq             | RrAxleLkIndRq                    | C                  | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      | JL |                 |                 | RrAxleLkIndRq                                                                                 | vehicle      | Rear axle lock indicator request                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                          |                                                                                            | FALSE       | TRUE         | RrAxleLkIndRq         | 256           | 1                  | RrAxleLkIndRq                    | state         | TYPE_INT    | 0             | 3             | 1          |                                          |
| 18 | VehCfg1.VC_SSC_Prsnt              | SelectSpeedControl               | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 | SelectSpeedControl                                                                            | device       | Tells if SSC is present on vehicle.   SelectSpeedControl sensor. It has one channel, which tells if the Select speed control feature is Present. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              |                                                                                            | FALSE       | TRUE         | VC_SSC_Prsnt          | 256           | 1                  | SelectSpeedControl               |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 13 | GW_C_I_11.SelSpdSts               | SelectSpeedStatus                | BH                 | 200                | 200                |   | On-change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF389           |                 | SelectSpeedStatus                                                                             | device       | SelectSpeedStatus sensor. It has one channel, which tells the Select speed status. This sensor cannot be switched off and is always available.0=OFF1=SELECT2=INHIBIT3=SNA                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 |                                                                                            | FALSE       | TRUE         | SelSpdSts             | 256           | 1                  | SelectSpeedStatus                |               | TYPE_INT    | 0             | 3             | 1          |                                          |
| 43 | ESP_B1.SelSpdLmp                  | SelSpdLmp                        | C                  | 50                 | 200                |   | On-change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | SelSpdLmp                                                                                     | device       | Select speed lamp status                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  |                                                                                            | FALSE       | TRUE         | SelSpdLmp             | 256           | 1                  | SelSpdLmp                        |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 41 | GW_C_I2.SHFT_PROG                 | SHFT_PROG                        | BH                 | 1000               | 1000               |   | On-change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | SHFT_PROG                                                                                     | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | SHFT_PROG             | 256           | 1                  | SHFT_PROG                        |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 40 | GW_C1.VEH_SPEED                   | Speedometer                      | BH                 | 100                | 100                |   | min,average,max                                        | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | Speedometer                                                                                   | vehicle      | Speedometer sensor is a range based component. It has one channel, which returns the vehicle speed. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | VEH_SPEED             | 256           | 1                  | Speedometer                      | range         | TYPE_DOUBLE | 0             | 511.9         | 0.0078125  | km/h                                     |
| 31 | GW_LIN_C_I2.SpeedUnit             | SpeedUnit                        | BH                 | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | SpeedUnit                                                                                     | device       | SpeedUnit sensor. It has one channel which tells you the Speed (speedometer) units. Miles = [1]. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              |                                                                                            | FALSE       | TRUE         | SpeedUnit             | 256           | 1                  | SpeedUnit                        |               | TYPE_INT    | 0             | 2             | 1          |                                          |
| 70 | ASBS_1.SwayBar_Sts                | SwayBar_Sts                      | C                  | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      | JL | VF640           |                 | SwayBar_Sts                                                                                   | vehicle      | Swaybar status: 0=Unlocked, 1=Locked, 2=S_I_P, 3= SNA                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     |                                                                                            | FALSE       | TRUE         | SwayBar_Sts           | 256           | 1                  | SwayBar_Sts                      | state         | TYPE_INT    | 0             | 3             | 1          | SwayBar_Sts: LOCKEDSwayBar_Sts: UNLOCKED |
| 71 | ASBS_1.SwayBarEVICDisplay         | SwayBarEVICDisplay               | C                  | 1000               | 1000               |   | Never                                                  |                                                    | Never                                                 | JL |                 |                 | SwayBarEVICDisplay                                                                            | vehicle      | Sway Bar HMI display request                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              |                                                                                            | FALSE       | TRUE         | SwayBarEVICDisplay    | 256           | 1                  | SwayBarEVICDisplay               | state         | TYPE_INT    | 0             | 15            | 1          |                                          |
| 45 | DTCM_B1.Tcase4Low                 | Tcase4Low                        | C                  | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | Tcase4Low                                                                                     | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | Tcase4Low             | 256           | 1                  | Tcase4Low                        |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 46 | DTCM_B1.TcaseNtrlStat             | none                             | C                  | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | TcaseNtrlStat                                                                                 | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | TcaseNtrlStat         | 256           | 1                  | TcaseNtrlStat                    |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 82 | TRNS_SPD.TCM_ManMd                | TCM_ManMd                        | C                  | 20                 | 200                |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      | JL |                 |                 | TCM_ManMd                                                                                     | vehicle      | Transmission in manual mode                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               |                                                                                            | FALSE       | TRUE         | TCM_ManMd             | 256           | 1                  | TCM_ManMd                        | state         | TYPE_INT    | 0             | 1             | 1          |                                          |
| 32 | GW_LIN_C_I2.TemperatureUnit       | TemperatureUnit                  | BH                 | 1000               | 1000               |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | TemperatureUnit                                                                               | device       | TemperatureUnit sensor. It has one channel which tells you the Temperature units. Farenheit = [1]. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            |                                                                                            | FALSE       | TRUE         | TemperatureUnit       | 256           | 1                  | TemperatureUnit                  |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 4  | GW_C_I3.TCASE_STAT                | TransferCaseStatus               | BH                 | 500                | 500                |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF737           |                 | TransferCaseStatus                                                                            | device       | TransferCaseStatus sensor. It has one channel, which tells if the Transfer Case Status. This sensor cannot be switched off and is always available.0=SH_IPG1=4LO2=4HI3=2WD4=N5=AUTO6=PT7=SNA                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              |                                                                                            | FALSE       | TRUE         | TCASE_STAT            | 256           | 1                  | TransferCaseStatus               |               | TYPE_INT    | 0             | 7             | 1          |                                          |
| 50 | TRNS_STAT2.TxTemp_Excess          | TransOverTemp                    | C                  | 100                | 500                |   | On change                                              | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    |                 |                 | TransOverTemp                                                                                 | vehicle      | TransOverTemp sensor is a state based component. It has one channel, which returns the TransOverTemp state.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               | 0,1                                                                                        | FALSE       | TRUE         | TxTemp_Excess         | 256           | 1                  | TransOverTemp                    | state         | TYPE_INT    | 0             | 1             | 1          |                                          |
| 26 | GW_C_I5.TX_TEMP                   | TX_TEMP                          | BH                 | 200                | 200                |   | min,average,max                                        | Configurable(10 sec <  Y < X ) Default: Y = 20 sec | Configurable(Default: X = 2 min)                      |    | VF690           |                 | TX_TEMP                                                                                       | device       | Transmission Temp                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         |                                                                                            | FALSE       | TRUE         | TX_TEMP               | 256           | 1                  | TX_TEMP                          |               | TYPE_INT    | -50           | 204           | 1          | °C                                       |
| 73 | VehCfg7.VC_AxleLockerPrsnt        | VC_AxleLockerPrsnt               | VC_AxleLockerPrsnt | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     | JL | VF639           |                 | VC_AxleLockerPrsnt                                                                            | vehicle      | Axle locker configurationVC_AxleLockerPrsnt = 0  (Vehicle not equipped with Locker)VC_AxleLockerPrsnt = 1(REAR)  (Vehicle equipped with Rear Locker Only)VC_AxleLockerPrsnt=2(FTRR) (Vehicle equipped with Front and Rear Lockers)                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        |                                                                                            | FALSE       | TRUE         | VC_AxleLockerPrsnt    | 256           | 1                  | VC_AxleLockerPrsnt               | state         | TYPE_INT    | 0             | 3             | 1          |                                          |
| 78 | VehCfg1.VC_BODY_STYLE             | VC_BODY_STYLE                    | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     | JL |                 |                 | VC_BODY_STYLE                                                                                 | vehicle      | Body style                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                |                                                                                            | FALSE       | TRUE         | VC_BODY_STYLE         | 256           | 1                  | VC_BODY_STYLE                    | state         | TYPE_INT    | 0             | 15            | 1          |                                          |
| 77 | VehCfg1.VC_LHD_RHD                | VC_LHD_RHD                       | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     | JL |                 |                 | VC_LHD_RHD                                                                                    | vehicle      | Left/right hand drive                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     |                                                                                            | FALSE       | TRUE         | VC_LHD_RHD            | 256           | 1                  | VC_LHD_RHD                       | state         | TYPE_INT    | 0             | 3             | 1          |                                          |
| 1  | VehCfg5.VC_OffRoadPg              | VC_OffRoadPg                     | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 | VC_OffRoadPg                                                                                  | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | VC_OffRoadPg          | 256           | 1                  | VC_OffRoadPg                     |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 56 | VehCfg2.VC_SpecialPKG_IC          | VC_SpecialPKG_IC                 | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 | VC_SpecialPKG_IC                                                                              | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | VC_SpecialPKG_IC      | 256           | 1                  | VC_SpecialPKG_IC                 |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 66 | VehCfg2.VC_SpecialPKG_IC          | VC_SpecialPKG_IC                 | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     | JL |                 |                 | VC_SpecialPKG_IC                                                                              | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | VC_SpecialPKG_IC      | 256           | 1                  | VC_SpecialPKG_IC                 |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 38 | VehCfg3.VC_SRT_PRSNT              | VC_SRT_PRSNT                     | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 | VC_SRT_PRSNT                                                                                  | device       | SRT Present sensor. It has one channel, which returns the SRT Present status.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             |                                                                                            | FALSE       | TRUE         | VC_SRT_PRSNT          | 256           | 1                  | VC_SRT_PRSNT                     |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 68 | VehCfg3.VC_TcaseTyp               | VC_TcaseTyp                      | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     | JL |                 | Not used        | VC_TcaseTyp                                                                                   | vehicle      | Transfer Case typeVC_TcaseType= Tcase_156 (Non Locking, only Auto and 2WD)VC_TcaseType= Tcase_256_3022 (Auto,4LO,N,SH_IPG)                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                |                                                                                            | FALSE       | TRUE         | VC_TcaseTyp           | 256           | 1                  | VC_TcaseTyp                      | state         | TYPE_INT    | 0             | 15            | 1          |                                          |
| 80 | VehCfg7.VC_Trans_Equipped         | VC_Trans_Equipped                | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     | JL |                 |                 | VC_Trans_Equipped                                                                             | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | VC_Trans_Equipped     | 256           | 1                  | VC_Trans_Equipped                |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 39 | VehCfg7.VC_TransType              | VC_TransType                     | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 | VC_TransType                                                                                  | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | VC_TransType          | 256           | 1                  | VC_TransType                     |               | TYPE_INT    | 0             | 63            | 1          |                                          |
| 42 | VehCfg3.VC_VEH_BRAND              | VC_VEH_BRAND                     | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 | VC_VEH_BRAND                                                                                  | device       | Vehicle Brand                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             |                                                                                            | FALSE       | TRUE         | VC_VEH_BRAND          | 256           | 1                  | VC_VEH_BRAND                     |               | TYPE_INT    | 0             | 15            | 1          |                                          |
| 37 | VehCfg1.VC_VEH_LINE               | VC_VEH_LINE                      | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 | VC_VEH_LINE                                                                                   | device       | Vehicle Line                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              |                                                                                            | FALSE       | TRUE         | VC_VEH_LINE           | 256           | 1                  | VC_VEH_LINE                      |               | TYPE_INT    | 0             | 256           | 1          |                                          |
| 57 | VehCfg1.VC_VehCfg1_Stat           | VC_VehCfg1_Stat                  | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 | WHY , not used? | VC_VehCfg1_Stat                                                                               | device       | Configuration messages status 1                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | VC_VehCfg1_Stat       | 256           | 1                  | VC_VehCfg1_Stat                  |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 58 | VehCfg2.VC_VehCfg2_Stat           | VC_VehCfg2_Stat                  | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 | WHY , not used? | VC_VehCfg2_Stat                                                                               | vehicle      | Configuration messages status 2                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | VC_VehCfg2_Stat       | 256           | 1                  | VC_VehCfg2_Stat                  | state         | TYPE_INT    | 0             | 2             | 1          |                                          |
| 59 | VehCfg3.VC_VehCfg3_Stat           | VC_VehCfg3_Stat                  | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 | WHY , not used? | VC_VehCfg3_Stat                                                                               | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | VC_VehCfg3_Stat       | 256           | 1                  | VC_VehCfg3_Stat                  |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 60 | VehCfg5.VC_VehCfg5_Stat           | none                             | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 | WHY , not used? | VC_VehCfg5_Stat                                                                               | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | VC_VehCfg5_Stat       | 256           | 1                  | VC_VehCfg5_Stat                  |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 61 | VehCfg7.VC_VehCfg7_Stat           | none                             | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 | WHY , not used? | VC_VehCfg7_Stat                                                                               | device       |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            | FALSE       | TRUE         | VC_VehCfg7_Stat       | 256           | 1                  | VC_VehCfg7_Stat                  |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 19 | VehCfg1.VC_XWD                    | VC_XWD                           | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | Configurable(Default: X = 2 min)                      |    |                 |                 | VC_XWD                                                                                        | device       | VC_XWD sensor. It has one channel which tells Drive configuration. This sensor cannot be switched off and is always available.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            |                                                                                            | FALSE       | TRUE         | VC_XWD                | 256           | 1                  | VC_XWD                           |               | TYPE_INT    | 0             | 3             | 1          |                                          |
| 64 | ECM_INDICATORS.EngOilIndLmp_On_Rq | WarningLightEvent                | C                  | 100                | 200                |   | Once (At HU app launch)                                |                                                    | Configurable(Default: X = 2 min)                      |    |                 |                 | WarningLightEvent                                                                             | device       | WarningLightEvent sensor. It has one channel, which returns the WarningLightEvent value.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  |                                                                                            | FALSE       | TRUE         | EngOilIndLmp_On_Rq    | 256           | 1                  | WarningLightEvent                |               | TYPE_INT    | 0             | 1             | 1          |                                          |
| 14 | NET_CFG_PT.NetCfg_ASCM            | NetCfg_ASCM                      | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    | VF440_V4, VF737 |                 |                                                                                               |              | Active Damping Control Module (1=present)                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 |                                                                                            |             |              |                       |               |                    |                                  |               |             |               |               |            |                                          |
| 15 | NET_CFG_PT.NetCfg_DTCM            | NetCfg_DTCM                      | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 |                                                                                               |              |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            |             |              |                       |               |                    |                                  |               |             |               |               |            |                                          |
| 16 | NET_CFG_PT.NetCfg_ELSD            | NetCfg_ELSD                      | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 |                 |                                                                                               |              | ELSD Locker Status                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        |                                                                                            |             |              |                       |               |                    |                                  |               |             |               |               |            |                                          |
| 34 | NET_CFG_PT.NetCfg_TCM             | NetCfg_TCM                       | BH                 | 2000               | 2000               |   | Once (At HU app launch)                                |                                                    | X                                                     |    |                 | WHY , not used? |                                                                                               |              |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            |             |              |                       |               |                    |                                  |               |             |               |               |            |                                          |
| 53 | Latitude                          | n/a                              | Internal           | n/a                | n/a                |   | Never (obtainable from TBM)                            |                                                    | X                                                     |    |                 |                 |                                                                                               |              |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            |             |              |                       |               |                    |                                  |               |             |               |               |            |                                          |
| 54 | Longitude                         | n/a                              | Internal           | n/a                | n/a                |   | Never (obtainable from TBM)                            |                                                    | X                                                     |    |                 |                 |                                                                                               |              |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            |             |              |                       |               |                    |                                  |               |             |               |               |            |                                          |
| 55 | Altitude                          | n/a                              | Internal           | n/a                | n/a                |   | Never (obtainable from TBM)                            |                                                    | X                                                     |    |                 |                 |                                                                                               |              |                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           |                                                                                            |             |              |                       |               |                    |                                  |               |             |               |               |            |                                          |
|    |                                   |                                  |                    |                    |                    |   |                                                        |                                                    |                                                       |    |                 |                 | VC_BODY_STYLE                                                                                 | state        | vehicle                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   | Body style                                                                                 |             | FALSE        | TRUE                  | VC_BODY_STYLE | 256                | 1                                | VC_BODY_STYLE | TYPE_INT    | 0             | 15            | 1          |                                          |
|    |                                   |                                  |                    |                    |                    |   |                                                        |                                                    |                                                       |    |                 |                 | VC_LHD_RHD                                                                                    | state        | vehicle                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   | Left/right hand drive                                                                      |             | FALSE        | TRUE                  | VC_LHD_RHD    | 256                | 1                                | VC_LHD_RHD    | TYPE_INT    | 0             | 3             | 1          |                                          |

To know more about the project:  

[SFS One Pagers](https://partners.chrysler.com/sites/ict-moparspcc/CVP/CVP%20Planning%20Assets/01.%20CVP%20Strategy%202017/01.%20GDSP%20RFP%20Restricted/13.%20Docs%20-%20Call%20Center%20Team/TBM%20SFS%20One_Pagers%20TK%207-26-17.pdf) is where you can find information for each service  
[R1 Feature Description](https://partners.chrysler.com/sites/ict-moparspcc/CVP/CVP%20Planning%20Assets/01.%20CVP%20Strategy%202017/01.%20GDSP%20RFP%20Restricted/13.%20Docs%20-%20Call%20Center%20Team/R1%20Feature%20Descriptions%208-8-17.pdf) is where you can find the Feature Detailed Description  

