Client Example Code (HU/TBM):

    /**********************************************************************************************
     * This example code is provided for illustrative purposes only and provided 'AS IS' without
     * warranty of any kind.
     *
     * Copyright ©2014 Chrysler Group LLC.  All Rights Reserved.  All information contained herein is,
     * and remains the property of Chrysler Group LLC and its suppliers, if any.  The intellectual and
     * technical concepts contained herein are proprietary to Chrysler Group LLC and its suppliers
     * and may be covered by U.S. and Foreign Patents, patents in process, and are protected by trade
     * secret or copyright law. Dissemination of this information or reproduction of this material is
     * strictly forbidden unless prior written permission is obtained from Chrysler Group LLC.
     *
     * Chrysler, Jeep, Dodge, Ram, SRT, Mopar and the Pentastar logo are registered trademarks of
     * Chrysler Group LLC. FIAT is a registered trademark of Fiat group Marketing & Corporate
     * Communication S.p.A. used under license by Chrysler Group LLC.
     *********************************************************************************************/
    package com.fca.uconnect.global;

    import com.amazonaws.services.iot.client.AWSIotException;
    import com.amazonaws.services.iot.client.AWSIotMessage;
    import com.amazonaws.services.iot.client.AWSIotMqttClient;
    import com.amazonaws.services.iot.client.AWSIotQos;
    import com.amazonaws.services.iot.client.AWSIotTopic;
    import com.fca.uconnect.global.GlobalUconnectControl.Location;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectAny;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectMessage;
    import com.fca.uconnect.global.GlobalUconnectExtTheftAlarmNotify.TheftAlarmNotification;
    import com.fca.uconnect.global.GlobalUconnectExtTheftAlarmNotify.TheftAlarmNotification.AlarmCause;
    import com.fca.uconnect.global.GlobalUconnectExtTheftAlarmNotify.TheftAlarmNotification.AlarmStatusEnum;
    import com.google.protobuf.ByteString;
    import com.google.protobuf.ExtensionRegistry;
    import com.google.protobuf.InvalidProtocolBufferException;

    /**
     * This example class demonstrates how to use the AWS IoT mqtt client to send a Uconnect TheftAlarmNotification message to the SDP and wait for a response message.
     * This code is only for reference and is furnished without warranty.....
     *
     * @author FCA Global V2C API Team
     *
     */
    public class TBMExampleForTheftAlarm {

    	private String clientId; // The clientId is unique to the device and obtained from the client X.509 certificate CN.
    	private ByteString sessionId; // The sessionId is assigned by the SDP to maintain a session independent of connection protocols.
    	private int messageId; // The messageId is a sequential number incremented and assigned to each message sent from the client.
    	private AWSIotMqttClient mqttClient; // The mqtt client object from the AWS IoT client library.
    	private boolean receivedResponse = false; // flag to wait for the response as part of this example.
    	private AWSIotTopic iotTopic; // The Topic object to subscribe for inbound messages.
    	private ExtensionRegistry extRegistry; // Google protocol buffers extension registry instance.

    	/**
    	 * Constructor - initialize protocol buffer extension registry for parsing incoming Uconnect Messages.
    	 */
    	public TBMExampleForTheftAlarm() {
    		extRegistry = ExtensionRegistry.newInstance();
    		extRegistry.add(GlobalUconnectExtTheftAlarmNotify.theftAlarmNotificationResponse);
    		extRegistry.add(GlobalUconnectExtTheftAlarmNotify.theftAlarmNotification);
    	}

    	/**
    	 * This method generates a Protocol Buffer Uconnect Message given the required inputs for TheftAlarmNotification.
    	 * @param alarmCause
    	 * @param vehicleLocation
    	 * @param alarmStatus
    	 * @return
    	 */
    	public UconnectMessage getTheftAlarmNotifyMsg(AlarmCause alarmCause,Location vehicleLocation,AlarmStatusEnum alarmStatus){

    		this.messageId++;
    		sessionId = ByteString.copyFrom(new byte[18]);
    		TheftAlarmNotification theftAlarmMsg = TheftAlarmNotification.newBuilder()
    				.setAlarmCause(alarmCause)
    				.setAlarmStatusEnum(alarmStatus)
    				.setVehicleLocation(vehicleLocation)
    				.setTimeStamp(System.currentTimeMillis())
    				.build();
    		UconnectMessage msg = UconnectMessage.newBuilder()
    			.setTimestamp(System.currentTimeMillis())
    			.setMessageId(messageId)
    			.addMessages(UconnectAny.newBuilder().
    			 setExtension(GlobalUconnectExtTheftAlarmNotify.theftAlarmNotification, theftAlarmMsg))
    			.build();

    		return msg;
    	}

    	/**
    	 * This method demonstrates connecting to the AWS IoT mqtt broker and publishing an TheftAlarmNotification message to the TANF topic.
    	 */
    	public void process() {

    		mqttClient = new AWSIotMqttClient("endpoint", clientId, "awsAccessKeyId", "awsSecretAccessKey");
    		try {
    			mqttClient.connect();

    			iotTopic = new AWSIotTopic(clientId+"/TANF/", AWSIotQos.QOS1) {
    				public void onMessage(AWSIotMessage msg) {
    					UconnectMessage msgIn;
    					try {
    						msgIn = UconnectMessage.parseFrom(msg.getPayload(),extRegistry);
    					} catch (InvalidProtocolBufferException e) {
    						e.printStackTrace();
    					}
    				}
    			};
    			mqttClient.subscribe(iotTopic);
    			AlarmCause alarmCause = AlarmCause.newBuilder()
    					.setIsFLDoorBreached(true)
    					.setIsVehiclePositionChanged(true)
    					.build();
    			Location vehicleLocation = Location.newBuilder()
    					.setPositionLongitude(43.9999f)
    					.setPositionLatitude(-84.54635343f)
    					.build();

    			UconnectMessage msg = getTheftAlarmNotifyMsg(alarmCause,vehicleLocation,AlarmStatusEnum.ACTIVE);
    			sendMessage(msg);

    		} catch (AWSIotException ex) {
    			System.out.println("Caught AWS Exception "+ex);
    			ex.printStackTrace();
    		}
    	}
    	/**
    	 * This method publishes the message to TANF topic
    	 */
    	public void sendMessage(UconnectMessage msg) {
    		final byte[] msgOut = msg.toByteArray();
    		new Thread(new Runnable() {

    		    @Override
    		public void run() {
    		try {
    			AWSIotMessage message = new
    					MessagePublisherListener("/TANF/"+clientId,AWSIotQos.QOS1,msgOut);
    			mqttClient.publish(message);

    		} catch (AWSIotException e) {
    			System.out.println("Caught Exception "+e);
    						e.printStackTrace();
    					}
    			    }
    			}).start();
    		}

    	/**
    	 * Example main to launch example.
    	 *
    	 */
    	public static void main(String[] args) {
    		TBMExampleForTheftAlarm example = new TBMExampleForTheftAlarm();
    		example.process();
    	}
    }

Here's an example of how Service Connects to AWS IOT MQTT for Theft AlarmNotification topics and process TheftAlarmNotification Request , send Acknowledgement.

Service Example Code (SDP):

    package com.fca.uconnect.global;

    import com.amazonaws.services.iot.client.AWSIotException;
    import com.amazonaws.services.iot.client.AWSIotMessage;
    import com.amazonaws.services.iot.client.AWSIotMqttClient;
    import com.amazonaws.services.iot.client.AWSIotQos;
    import com.amazonaws.services.iot.client.AWSIotTopic;

    import com.fca.uconnect.global.GlobalUconnectControl.UconnectMessage;
    import com.google.protobuf.ByteString;
    import com.google.protobuf.ExtensionRegistry;

    public class SDPExampleForTheftAlarm {
    private String clientId; // The clientId is unique to the device and obtained from the client X.509 certificate CN.
    private ByteString sessionId; // The sessionId is assigned by the SDP to maintain a session independent of connection protocols.
    private int messageId; // The messageId is a sequential number incremented and assigned to each message sent from the client.
    private AWSIotMqttClient mqttClient; // The mqtt client object from the AWS IoT client library.
    private AWSIotTopic iotTopic; // The Topic object to subscribe for inbound messages.
    private ExtensionRegistry extRegistry; // Google protocol buffers extension registry instance.
    private Semaphore semaphore;//The semaphore object is used to wait for a response.

    public SDPExampleForTheftAlarm() {
    	extRegistry = ExtensionRegistry.newInstance();
    	extRegistry.add(GlobalUconnectExtTheftAlarmNotify.theftAlarmNotification);
    	this.semaphore = new Semaphore();
    }

    public void process() {
    mqttClient = new AWSIotMqttClient("endpoint", clientId, "awsAccessKeyId", "awsSecretAccessKey");

    try {
    mqttClient.connect();
     iotTopic = new AWSIotTopic("/TANF/#",AWSIotQos.QOS1){
    	public void onMessage(AWSIotMessage msg) {
    try {
    	UconnectMessage	msgIn = UconnectMessage.parseFrom(msg.getPayload(),extRegistry);
    	if(msgIn.getMessages(0).hasExtension(GlobalUconnectExtTheftAlarmNotify.theftAlarmNotification)){
    		semaphore.unlock();
         }

    } catch( Exception ex) {
    	ex.printStackTrace();
    	System.out.println("Err processing message: "+ex+", try parsing Theft Alarm Notification.");
    }
    }
    };
    mqttClient.subscribe(iotTopic);

    } catch (AWSIotException e) {
    	System.out.println("Caught Exception "+e);
    	e.printStackTrace();
    }

    try {
    	this.semaphore.lock();// lock thread
    } catch (InterruptedException e) {

    }
    }

    public void sendMessage(UconnectMessage msg) {
    final byte[] msgOut = msg.toByteArray();
    new Thread(new Runnable() {

        @Override
    public void run() {
    try {
    	AWSIotMessage message = new
    			MessagePublisherListener(clientId+"/TANF/",AWSIotQos.QOS1,msgOut);
    	mqttClient.publish(message);
    } catch (AWSIotException e) {
    	System.out.println("Caught Exception "+e);
    				e.printStackTrace();
    			}
    	    }
    	}).start();
    }
    public static void main(String[] args) {
    	SDPExampleForTheftAlarm m = new SDPExampleForTheftAlarm();
    	m.process();
    }
    }

The example code demonstrates how to connect with AWS IoT for publishing and subscribing to the Theft Alarm Notification topic.

Download Client Example Code here

Download Service Example Code here