    /**********************************************************************************************
     * This example code is provided for illustrative purposes only and provided 'AS IS' without
     * warranty of any kind.
     *
     * Copyright ©2014 Chrysler Group LLC.  All Rights Reserved.  All information contained herein is,
     * and remains the property of Chrysler Group LLC and its suppliers, if any.  The intellectual and
     * technical concepts contained herein are proprietary to Chrysler Group LLC and its suppliers
     * and may be covered by U.S. and Foreign Patents, patents in process, and are protected by trade
     * secret or copyright law. Dissemination of this information or reproduction of this material is
     * strictly forbidden unless prior written permission is obtained from Chrysler Group LLC.
     *
     * Chrysler, Jeep, Dodge, Ram, SRT, Mopar and the Pentastar logo are registered trademarks of
     * Chrysler Group LLC. FIAT is a registered trademark of Fiat group Marketing & Corporate
     * Communication S.p.A. used under license by Chrysler Group LLC.
     *********************************************************************************************/
    package com.fca.uconnect.global;
    import java.util.List;
    import com.amazonaws.services.iot.client.AWSIotException;
    import com.amazonaws.services.iot.client.AWSIotMessage;
    import com.amazonaws.services.iot.client.AWSIotMqttClient;
    import com.amazonaws.services.iot.client.AWSIotQos;
    import com.amazonaws.services.iot.client.AWSIotTopic;
    import com.fca.uconnect.global.GlobalUconnectControl.Location;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectAny;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectMessage;
    import com.fca.uconnect.global.GlobalUconnectExtPC.PCNotificationPublish;
    import com.fca.uconnect.global.GlobalUconnectExtPC.PCNotificationPublish.NotificationType;
    import com.fca.uconnect.global.GlobalUconnectExtPC.PCNotificationPublish.SignalSource;
    import com.fca.uconnect.global.GlobalUconnectExtPC.PCNotificationPublish.VehiclePosition;
    import com.fca.uconnect.global.GlobalUconnectExtPC.PCUpdateConfigResponse;
    import com.fca.uconnect.global.GlobalUconnectExtPC.PCUpdateConfigResponse.ResponseEnum;
    import com.fca.uconnect.global.GlobalUconnectExtRoadSideAssist.RSADataUpload.EngineStatusEnum;
    import com.fca.uconnect.global.GlobalUconnectExtRoadSideAssist.RSADataUpload.ErrorTellTale;
    import com.fca.uconnect.global.GlobalUconnectExtRoadSideAssist.RSADataUpload.TirePressure;
    import com.fca.uconnect.global.util.MessageUtil;
    import com.google.protobuf.ByteString;
    import com.google.protobuf.ExtensionRegistry;
    import com.google.protobuf.InvalidProtocolBufferException;

    /**
     * This example class demonstrates how to use the AWS IoT mqtt client to send a Uconnect RoadSideAsistance message with Data to the SDP .
     * This code is only for reference and is furnished without warranty.....
     *
     * @author FCA Global V2C API Team
     *
     */
    public class TBMExampleForPC {

    	private String clientId; // The clientId is unique to the device and obtained from the client X.509 certificate CN.
    	private int messageId; // The messageId is a sequential number incremented and assigned to each message sent from the client.
    	private AWSIotMqttClient mqttClient; // The mqtt client object from the AWS IoT client library.
    	private AWSIotTopic iotTopic; // The Topic object to subscribe for inbound messages.
    	private ExtensionRegistry extRegistry; // Google protocol buffers extension registry instance.
    	List messages ;

    	/**
    	 * Constructor - initialize protocol buffer extension registry for parsing incoming Uconnect Messages.
    	 */
    	public TBMExampleForPC() {
    		extRegistry = ExtensionRegistry.newInstance();
    		extRegistry.add(GlobalUconnectExtPC.pcUpdateConfigRequest);
    	}

    	/**
    	 * This method generates a Protocol Buffer Uconnect Message given the required inputs for Parental Control Response
    	 * @param ResponseEnum
    	 * @return
    	 */
    	public UconnectMessage getPCConfigRespMsg(ResponseEnum respEnum) {
    		this.messageId++;
    		PCUpdateConfigResponse pcConfigResp = PCUpdateConfigResponse.newBuilder()
    				.setResponseEnum(respEnum)
    				.build();
    		UconnectMessage msg = UconnectMessage.newBuilder()
    			.setTimestamp(System.currentTimeMillis())
    			.setMessageId(messageId)
    			.addMessages(UconnectAny.newBuilder().
    			 setExtension(GlobalUconnectExtPC.pcUpdateConfigResponse, pcConfigResp))
    			.build();
    		return msg;
    	}
    	public UconnectMessage getPCNotifyPubMsg() {
    		this.messageId++;
    		Location vehicleLocation = Location.newBuilder()
    				.setPositionLongitude(43.9999f)
    				.setPositionLatitude(-84.54635343f)
    				.build();
    		VehiclePosition vehPosition = VehiclePosition.newBuilder()
    			.setPositionEncrypted(false)
    			.setGpsTimestamp((int)System.currentTimeMillis())
    			.setVehicleDirection(32)
    			.setVehiclePosition(vehicleLocation)
    			.build();
    		PCNotificationPublish notify = PCNotificationPublish.newBuilder()
    				.setAcceleration(35)
    				.setNotificatonType(NotificationType.SUDDEN_CORNERING)
    				.setSpeed(75)
    				.setSteeringWheelRotationRate(15.5f)
    				.setVehiclePosition(vehPosition)
    				.setSpeedSource(SignalSource.TBM_ACCELEROMETER)
    				.setAccelerationSource(SignalSource.TBM_ACCELEROMETER)
    				.build();
    		UconnectMessage msg = UconnectMessage.newBuilder()
    			.setTimestamp(System.currentTimeMillis())
    			.setMessageId(messageId)
    			.addMessages(UconnectAny.newBuilder().
    			 setExtension(GlobalUconnectExtPC.pcNotificationPublish, notify))
    			.build();
    		return msg;
    	}

    	/**
    	 * This method demonstrates connecting to the AWS IoT mqtt broker and publishing an RSADataUpload message to the RSA topic.
    	 */
    	public void process() {

    		mqttClient = new AWSIotMqttClient("endpoint", clientId, "awsAccessKeyId", "awsSecretAccessKey");
    		try {
    			mqttClient.connect();
    			iotTopic = new AWSIotTopic(clientId+"/PC/", AWSIotQos.QOS1) {
    				public void onMessage(AWSIotMessage msg) {
    					UconnectMessage msgIn = null;
    					try {
    						msgIn = UconnectMessage.parseFrom(msg.getPayload(),extRegistry);
    					} catch (InvalidProtocolBufferException e) {
    					}
    					if(msgIn.getMessages(0).hasExtension(GlobalUconnectExtPC.pcUpdateConfigRequest)){
    						GlobalUconnectExtPC.PCUpdateConfigRequest pcConfigReq = msgIn.getMessages(0).getExtension(GlobalUconnectExtPC.pcUpdateConfigRequest);
    					UconnectMessage respMsg = getPCConfigRespMsg(ResponseEnum.SUCCESS);
    					sendMessage(respMsg);
    					sendMessage(getPCNotifyPubMsg());
    				}
    			}};
    			mqttClient.subscribe(iotTopic);
    		} catch (AWSIotException ex) {
    			System.out.println("Caught AWS Exception "+ex);
    			ex.printStackTrace();
    		}  catch (Exception e) {
    			e.printStackTrace();
    		}
    	}
    	/**
    	 * This method publishes the message to PC topic
    	 */
    	public void sendMessage(UconnectMessage msg) {
    		final byte[] msgOut = msg.toByteArray();
    		new Thread(new Runnable() {

    		    @Override
    		public void run() {
    		try {
    			AWSIotMessage message = new
    					MessagePublisherListener("/PC/"+clientId,AWSIotQos.QOS1,msgOut);
    			mqttClient.publish(message);
    		} catch (AWSIotException e) {
    			System.out.println("Caught Exception "+e);
    						e.printStackTrace();
    					}
    			    }
    			}).start();
    		}

    	/**
    	 * Example main to launch example.
    	 *
    	 * @param args
    	 */
    	public static void main(String[] args) {
    		TBMExampleForPC example = new TBMExampleForPC();
    		example.process();
    	}
    }

Here's an example of how SDP Connects to AWS IOT MQTT for PC topics.

Service Example Code (SDP):

    package com.fca.uconnect.global;
    import java.util.ArrayList;
    import java.util.List;

    import com.amazonaws.services.iot.client.AWSIotException;
    import com.amazonaws.services.iot.client.AWSIotMessage;
    import com.amazonaws.services.iot.client.AWSIotMqttClient;
    import com.amazonaws.services.iot.client.AWSIotQos;
    import com.amazonaws.services.iot.client.AWSIotTopic;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectAny;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectMessage;
    import com.fca.uconnect.global.GlobalUconnectExtPC.PCUpdateConfigRequest;
    import com.fca.uconnect.global.GlobalUconnectExtPC.PCUpdateConfigRequest.ConfigTypeVehicle;
    import com.fca.uconnect.global.GlobalUconnectExtPC.PCUpdateConfigRequest.ConfigTypeVehicle.SpeedAlertConfig;
    import com.fca.uconnect.global.util.MessageUtil;
    import com.google.protobuf.ExtensionRegistry;

    public class SDPExampleForPC {
    private String clientId; // The clientId is unique to the device and obtained from the client X.509 certificate CN.
    private int messageId; // The messageId is a sequential number incremented and assigned to each message sent from the client.
    private AWSIotMqttClient mqttClient; // The mqtt client object from the AWS IoT client library.
    private AWSIotTopic iotTopic; // The Topic object to subscribe for inbound messages.
    private ExtensionRegistry extRegistry; // Google protocol buffers extension registry instance.
    private List messages;

    public SDPExampleForPC() {
    	extRegistry = ExtensionRegistry.newInstance();
    	extRegistry.add(GlobalUconnectExtPC.pcUpdateConfigResponse);
    }
    public UconnectMessage getPCConfigReqMsg() {
    	messageId++;
    	List activeDays = new ArrayList();
    	activeDays.add(1);
    	activeDays.add(2);
    	SpeedAlertConfig speedAlertMsg =SpeedAlertConfig.newBuilder()
    			.setBeginTime(1000)
    			.setEndTime(10000)
    			.setThresholdAbovePostedSpeed(60)
    			.setThresholdAbsolute(70)
    			.setThresholdPostedSpeedAbsent(80)
    			.addAllActiveDaysOfWeek(activeDays)
    			.build();
    	ConfigTypeVehicle configTypeVehicle = ConfigTypeVehicle.newBuilder()
    			.setUpdateSpeedAlertConfig(true)
    			.addSpeedAlerts(speedAlertMsg)
    			.build();
    	PCUpdateConfigRequest pcUpdateConfigReq = PCUpdateConfigRequest.newBuilder()
    			.setConfigTypeVehicle(configTypeVehicle)
    			.build();

    	UconnectMessage msg = UconnectMessage.newBuilder()
    		.setTimestamp(System.currentTimeMillis())
    		.setMessageId(messageId)
    		.addMessages(UconnectAny.newBuilder().
    		 setExtension(GlobalUconnectExtPC.pcUpdateConfigRequest,pcUpdateConfigReq ))
    		.build();

    	return msg;
    }
    /**
     * This method demonstrates connecting to the AWS IoT mqtt broker and Subscribing  an Parental Control message to the PC topic.
     */
    public void process() {

    	mqttClient = new AWSIotMqttClient("endpoint", clientId, "awsAccessKeyId", "awsSecretAccessKey");
    try {
    mqttClient.connect();
     iotTopic = new AWSIotTopic("/PC/#",AWSIotQos.QOS1){
    	public void onMessage(AWSIotMessage msg) {
    try {
    	UconnectMessage	msgIn = UconnectMessage.parseFrom(msg.getPayload(),extRegistry);
    	if(msgIn.getMessages(0).hasExtension(GlobalUconnectExtPC.pcUpdateConfigResponse)){
    		GlobalUconnectExtPC.PCUpdateConfigResponse pcConfigResp = msgIn.getMessages(0).getExtension(GlobalUconnectExtPC.pcUpdateConfigResponse);
    		if(messages==null)
    			messages = new ArrayList();
    		messages.add(msgIn.getMessages(0));
    	}
    } catch( Exception ex) {
    	ex.printStackTrace();
    }
    }
    };
    sendMessage(getPCConfigReqMsg());
    mqttClient.subscribe(iotTopic);

    } catch (AWSIotException e) {
    	System.out.println("Caught Exception "+e);
    	e.printStackTrace();
    }
    }

    public void sendMessage(UconnectMessage msg) {
    final byte[] msgOut = msg.toByteArray();
    new Thread(new Runnable() {

        @Override
    public void run() {
    try {
    	AWSIotMessage message = new
    			MessagePublisherListener(clientId+"/PC/",AWSIotQos.QOS1,msgOut);
    	mqttClient.publish(message);

    } catch (AWSIotException e) {
    	System.out.println("Caught Exception "+e);
    				e.printStackTrace();
    			}
    	    }
    	}).start();
    }
    public static void main(String[] args) {
    	SDPExampleForPC m = new SDPExampleForPC();
    	m.process();
    }
    }

The example code demonstrates how to connect with AWS IoT for publishing and subscribing to the Parental Control topic.

Download Client Example Code here

Download Service Example Code here