Client Example Code (HU/TBM):

    /**********************************************************************************************
     * This example code is provided for illustrative purposes only and provided 'AS IS' without
     * warranty of any kind.
     *
     * Copyright ©2014 Chrysler Group LLC.  All Rights Reserved.  All information contained herein is,
     * and remains the property of Chrysler Group LLC and its suppliers, if any.  The intellectual and
     * technical concepts contained herein are proprietary to Chrysler Group LLC and its suppliers
     * and may be covered by U.S. and Foreign Patents, patents in process, and are protected by trade
     * secret or copyright law. Dissemination of this information or reproduction of this material is
     * strictly forbidden unless prior written permission is obtained from Chrysler Group LLC.
     *
     * Chrysler, Jeep, Dodge, Ram, SRT, Mopar and the Pentastar logo are registered trademarks of
     * Chrysler Group LLC. FIAT is a registered trademark of Fiat group Marketing & Corporate
     * Communication S.p.A. used under license by Chrysler Group LLC.
     *********************************************************************************************/
    package com.fca.uconnect.global;

    import java.util.List;

    import com.amazonaws.services.iot.client.AWSIotException;
    import com.amazonaws.services.iot.client.AWSIotMessage;
    import com.amazonaws.services.iot.client.AWSIotMqttClient;
    import com.amazonaws.services.iot.client.AWSIotQos;
    import com.amazonaws.services.iot.client.AWSIotTopic;
    import com.fca.uconnect.global.GlobalUconnectControl.Location;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectAny;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectMessage;
    import com.fca.uconnect.global.GlobalUconnectExtRoadSideAssist.RSADataUpload;
    import com.fca.uconnect.global.GlobalUconnectExtRoadSideAssist.RSADataUpload.EngineStatusEnum;
    import com.fca.uconnect.global.GlobalUconnectExtRoadSideAssist.RSADataUpload.ErrorTellTale;
    import com.fca.uconnect.global.GlobalUconnectExtRoadSideAssist.RSADataUpload.TirePressure;
    import com.google.protobuf.ByteString;
    import com.google.protobuf.ExtensionRegistry;

    /**
     * This example class demonstrates how to use the AWS IoT mqtt client to send a Uconnect RoadSideAsistance message with Data to the SDP .
     * This code is only for reference and is furnished without warranty.....
     *
     * @author FCA Global V2C API Team
     *
     */
    public class TBMExampleForRSA {

    	private String clientId; // The clientId is unique to the device and obtained from the client X.509 certificate CN.
    	private ByteString sessionId; // The sessionId is assigned by the SDP to maintain a session independent of connection protocols.
    	private int messageId; // The messageId is a sequential number incremented and assigned to each message sent from the client.
    	private AWSIotMqttClient mqttClient; // The mqtt client object from the AWS IoT client library.
    	private AWSIotTopic iotTopic; // The Topic object to subscribe for inbound messages.
    	private ExtensionRegistry extRegistry; // Google protocol buffers extension registry instance.

    	List messages ;

    	/**
    	 * Constructor - initialize protocol buffer extension registry for parsing incoming Uconnect Messages.
    	 */
    	public TBMExampleForRSA() {
    		extRegistry = ExtensionRegistry.newInstance();
    		extRegistry.add(GlobalUconnectExtRoadSideAssist.rsaDataUpload);
    	}

    	/**
    	 * This method generates a Protocol Buffer Uconnect Message given the required inputs for RoadSideAssistance Data upload
    	 * @param location
    	 * @param tirePressure
    	 * @param errorTellTale
    	 * @param statusEnum
    	 * @param fuelLevel
    	 * @return
    	 */
    	public UconnectMessage getRSADataMsg(Location location,TirePressure tirePressure,ErrorTellTale errorTellTale , EngineStatusEnum statusEnum,float fuelLevel) {
    		this.messageId++;
    		sessionId = ByteString.copyFrom(new byte[18]);
    		RSADataUpload rsaData = RSADataUpload.newBuilder()
    				.setErrorTellTale(errorTellTale)
    				.setFuelLevel(fuelLevel)
    				.setTirePressure(tirePressure)
    				.setVehicleLocation(location)
    				.setEngineStatusEnum(statusEnum)
    				.build();
    		UconnectMessage msg = UconnectMessage.newBuilder()
    			.setTimestamp(System.currentTimeMillis())
    			.setMessageId(messageId)
    			.addMessages(UconnectAny.newBuilder().
    			 setExtension(GlobalUconnectExtRoadSideAssist.rsaDataUpload, rsaData))
    			.build();
    		return msg;
    	}

    	/**
    	 * This method demonstrates connecting to the AWS IoT mqtt broker and publishing an RSADataUpload message to the RSA topic.
    	 */
    	public void process() {

    		mqttClient = new AWSIotMqttClient("endpoint", clientId, "awsAccessKeyId", "awsSecretAccessKey");
    		try {
    			mqttClient.connect();

    			iotTopic = new AWSIotTopic(clientId+"/RSA/", AWSIotQos.QOS1) {
    				public void onMessage(AWSIotMessage msg) {
    					// You can receive messages if SDP sends any
    				}
    			};
    			mqttClient.subscribe(iotTopic);
    			Location carLocation = Location.newBuilder()
    					.setPositionLongitude(43.9999)
    					.setPositionLatitude(-84.54635343f)
    					.build();
    			TirePressure tirePressureMsg = TirePressure.newBuilder()
    					.setFlTirePressure(35)
    					.setFrTirePressure(34)
    					.setRlTirePressure(36)
    					.setRrTirePressure(35)
    					.build();
    			ErrorTellTale tellTaleMsg = ErrorTellTale.newBuilder()
    					.setIsOilPressure(true)
    					.build();
    			EngineStatusEnum engineStatus = EngineStatusEnum.REQUESTSTART;
    			UconnectMessage msg = getRSADataMsg(carLocation,tirePressureMsg,tellTaleMsg,engineStatus,20f);
    			mqttClient.publish("/RSA/"+clientId, AWSIotQos.QOS1, msg.toByteArray());

    		} catch (AWSIotException ex) {
    			System.out.println("Caught AWS Exception "+ex);
    			ex.printStackTrace();
    		}  catch (Exception e) {
    			e.printStackTrace();
    		}
    	}

    	/**
    	 * Example main to launch example.
    	 *
    	 * @param args
    	 */
    	public static void main(String[] args) {
    		TBMExampleForRSA example = new TBMExampleForRSA();
    		example.process();
    	}
    }

Here's an example of how Service Connects to AWS IOT MQTT for RSA topics and process RSADataUpload Request .

Service Example Code (SDP):

    package com.fca.uconnect.global;
    import com.amazonaws.services.iot.client.AWSIotException;
    import com.amazonaws.services.iot.client.AWSIotMessage;
    import com.amazonaws.services.iot.client.AWSIotMqttClient;
    import com.amazonaws.services.iot.client.AWSIotQos;
    import com.amazonaws.services.iot.client.AWSIotTopic;
    import com.fca.uconnect.global.GlobalUconnectControl.UconnectMessage;
    import com.google.protobuf.ByteString;
    import com.google.protobuf.ExtensionRegistry;

    public class SDPExampleForRSA {
    private String clientId; // The clientId is unique to the device and obtained from the client X.509 certificate CN.
    private ByteString sessionId; // The sessionId is assigned by the SDP to maintain a session independent of connection protocols.
    private int messageId; // The messageId is a sequential number incremented and assigned to each message sent from the client.
    private AWSIotMqttClient mqttClient; // The mqtt client object from the AWS IoT client library.
    private AWSIotTopic iotTopic; // The Topic object to subscribe for inbound messages.
    private ExtensionRegistry extRegistry; // Google protocol buffers extension registry instance.

    public SDPExampleForRSA() {
    	extRegistry = ExtensionRegistry.newInstance();
    	extRegistry.add(GlobalUconnectExtRoadSideAssist.rsaDataUpload);
    }
    public static void main(String[] args) {
    	SDPExampleForRSA m = new SDPExampleForRSA();
    	m.process();
    }
    /**
     * This method demonstrates connecting to the AWS IoT mqtt broker and Subscribing  an RSADataUpload message to the RSA topic.
     */
    public void process() {

    	mqttClient = new AWSIotMqttClient("endpoint", clientId, "awsAccessKeyId", "awsSecretAccessKey");

    try {
    mqttClient.connect();
     iotTopic = new AWSIotTopic("/RSA/#",AWSIotQos.QOS1){
    	public void onMessage(AWSIotMessage msg) {
    try {

    	UconnectMessage	msgIn = UconnectMessage.parseFrom(msg.getPayload(),extRegistry);

    	GlobalUconnectExtRoadSideAssist.RSADataUpload rsaDataMsg = msgIn.getMessages(0).getExtension(GlobalUconnectExtRoadSideAssist.rsaDataUpload);
    	//Receive Car data for RoadSide Assistance.

    } catch( Exception ex) {
    	ex.printStackTrace();
    }
    }
    };

    mqttClient.subscribe(iotTopic);
    } catch (AWSIotException e) {
    	System.out.println("Caught Exception "+e);
    	e.printStackTrace();
    }
    }
    }

The example code demonstrates how to connect with AWS IoT for publishing and subscribing to the RSA topic.

Download Client Example Code here

Download Service Example Code here